{"text_format":"3","workbook":"xlsx","n_sheets":5,"sheets":["CHECKLIST RATING 1","reting","FORM RATING","Data","Sheet2"],"not_rendered":{"images":11,"macros":1,"external_links":1,"defined_names":58},"read":"whole","date_system":"1900"}

{"sheet":"CHECKLIST RATING 1","index":0,"n_rows":85,"n_cols":17,"rows_kept":85,"hidden":true,"merged":[[2,1,2,4],[2,6,2,10],[2,12,2,17],[3,7,3,8],[3,14,3,15],[16,1,16,4],[16,12,16,17],[17,14,17,15],[19,6,19,10],[20,7,20,8],[24,12,24,17],[25,14,25,15],[28,6,28,10],[29,7,29,8],[50,6,50,10],[51,7,51,8],[55,12,55,17],[56,14,56,15]]}
[]
[]
[null," LHRA Factor and Max. Hazard Rating",{"$nulls":10},"Sub-Factor for Erotion"]
[null,null,"Factor","Max. Hazard Rating",null,null,"Sub-Factor","Variable",null,"Rating",{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[null,null,"Lithology",{"v":6,"d":"6.00"},null,null,"Lithology","Rock Type","Quartzite and limestone",{"v":0.6,"d":"0.60"},{"$nulls":3},"Erotion","No appreciable erosion","No appreciable erosion",{"v":0.2,"d":"0.20"}]
[null,null,"Degree of weathering",{"v":4,"d":"4.00"},{"$nulls":4},"Granite and gabbro",{"v":0.9,"d":"0.90"},{"$nulls":4},"Sheet erosion","Minor",{"v":0.6,"d":"0.60"}]
[null,null,"Structure",{"v":4,"d":"4.00"},{"$nulls":4},"Gneiss",{"v":1.2,"d":"1.20"},{"$nulls":5},"Moderate",{"v":0.8,"d":"0.80"}]
[null,null,"Slope condition",{"v":6,"d":"6.00"},{"$nulls":4},"Well-cemented ferrigenuous sedimentary rocks,dominantly sandstones with minor beds of claystone",{"v":3,"d":"3.00"},{"$nulls":5},"Severe",{"v":1,"d":"1.00"}]
[null,null,"Hydrology",{"v":6,"d":"6.00"},{"$nulls":4},"Poorly cemented terrigenuous sedimentary rocks, dominantly sand with clayey shale beds",{"v":4,"d":"4.00"},{"$nulls":4},"Rill erosion","Minor",{"v":0.6,"d":"0.60"}]
[null,null,"Erosion",{"v":4,"d":"4.00"},{"$nulls":4},"Salt and phyllite",{"v":3.6,"d":"3.60"},{"$nulls":5},"Moderate",{"v":0.8,"d":"0.80"}]
[null,null,"Physical / engineering properties",{"v":4,"d":"4.00"},{"$nulls":4},"Schist",{"v":4,"d":"4.00"},{"$nulls":5},"Severe",{"v":1,"d":"1.00"}]
[null,null,"Land use and land cover",{"v":4,"d":"4.00"},{"$nulls":4},"Shale with interbeded sandstone and quartzite",{"v":5.4,"d":"5.40"},{"$nulls":4},"Gully erosion","Minor",{"v":1.2,"d":"1.20"}]
[null,null,"Slope history",{"v":2,"d":"2.00"},{"$nulls":4},"Highly weathered shale, phyllite and schist typically with 60% of salt",{"v":6,"d":"6.00"},{"$nulls":5},"Moderate",{"v":1.6,"d":"1.60"}]
[null,null,"Total",{"$f":"SUM(D5:D13)","v":{"v":40,"d":"40.00"}},{"$nulls":3},"Soil Type","Older well-compacted fluvial fill material (alluvial)",{"v":2.4,"d":"2.40"},{"$nulls":5},"Severe",{"v":2,"d":"2.00"}]
[{"$nulls":8},"Clayey soil with naturally formed surface (eluvial)",{"v":3,"d":"3.00"}]
[{"$nulls":8},"Sandy soil with naturally formed surface (alluvial) Debris comprising mostly rock pieces mixed with clayey / sandy soil (colluvial):",{"v":4.2,"d":"4.20"}]
[null," Hazard values and ratings ",{"$nulls":6},"Older well compacted sandy soil",{"v":5,"d":"5.00"},null,null,"Sub-Factor for Slope Cover"]
[null,null,"Hazard ratings","Hazard values",{"$nulls":4},"Younger loose material sandy soil or mining material",{"v":6,"d":"6.00"},{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[null,null,"Very High Hazard","> 32.0",{"$nulls":9},"Slope Cover",null,"Thickly vegetated area",{"v":1,"d":"1.00"}]
[null,null,"High Hazard","26.6 – 31.9",{"$nulls":11},"Moderately vegetated area",{"v":2,"d":"2.00"}]
[null,null,"Moderate Hazard","20.4 – 26.5",null,null,"Sub-Factor","Variable",null,"Rating",{"$nulls":5},"Artificially and vegetated area",{"v":2.2,"d":"2.20"}]
[null,null,"Low Hazard","14.1 – 20.3",null,null,"Degree of weathering",null,"Fresh",{"v":0.6,"d":"0.60"},{"$nulls":5},"Artificial covers",{"v":2,"d":"2.00"}]
[null,null,"Very Low Hazard","< 14.0",{"$nulls":4},"Slightly weathered",{"v":1.2,"d":"1.20"},{"$nulls":5},"No cover",{"v":4,"d":"4.00"}]
[{"$nulls":8},"Moderately weathered",{"v":1.8,"d":"1.80"}]
[{"$nulls":8},"Highly weathered",{"v":2.4,"d":"2.40"},null,null,"Sub-Factor for Physical Properties"]
[{"$nulls":8},"Extremely weathered",{"v":3,"d":"3.00"},{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[{"$nulls":8},"Residual soil",{"v":4,"d":"4.00"},{"$nulls":3},"Physical properties ","Value of c (kN/m2)","No",0]
[{"$nulls":13},"of Soil slope;",null,"< 6 kN/m2",{"v":0.8,"d":"0.80"}]
[{"$nulls":15},"6 - 12 kN/m2",{"v":1,"d":"1.00"}]
[{"$nulls":6},"Sub-Factor","Variable",null,"Rating",{"$nulls":5},"12 - 18 kN/m2",{"v":1.2,"d":"1.20"}]
[{"$nulls":6},"Structure","Spacing of","> 2m",{"v":0.2,"d":"0.20"},{"$nulls":5},"> 18 kN/m2",{"v":1.4,"d":"1.40"}]
[{"$nulls":7},"discontinuities;","0.6m – 2m",{"v":0.4,"d":"0.40"},{"$nulls":4},"Plasticity index","No",{"v":0,"d":"0.00"}]
[{"$nulls":8},"200 mm – 600 mm",{"v":0.6,"d":"0.60"},{"$nulls":5},"< 10",{"v":0.8,"d":"0.80"}]
[{"$nulls":8},"60 mm – 200 mm",{"v":0.8,"d":"0.80"},{"$nulls":5}," 10 - 23 ",{"v":1.2,"d":"1.20"}]
[{"$nulls":8},"< 60 mm",{"v":1,"d":"1.00"},{"$nulls":5},"24 - 35",{"v":1.2,"d":"1.20"}]
[{"$nulls":7},"Width and continuity","Very rough surface. Not continuous. No separation. Unweathered wall rock.",{"v":0.2,"d":"0.20"},{"$nulls":5},"> 35 ",{"v":1.4,"d":"1.40"}]
[{"$nulls":7},"of joints","Slightly rough surface. Separation < 1mm.Slightly weathered wall.",{"v":0.4,"d":"0.40"},{"$nulls":4},"Angle of friction (degrees)","No",{"v":0,"d":"0.00"}]
[{"$nulls":8},"Slightly rough surface. Separation < 1mm.Highly weathered wall",{"v":0.6,"d":"0.60"},{"$nulls":5}," 0 - 11 °",{"v":0.8,"d":"0.80"}]
[{"$nulls":8},"Slickensided surface. OR Gouge < 5mm thick OR Separation 1 - 5mm continuous.",{"v":0.8,"d":"0.80"},{"$nulls":5},"12 - 23 °",{"v":1,"d":"1.00"}]
[{"$nulls":8},"Soft Gough > 5mm OR Separation > 5mm continuous.",{"v":1,"d":"1.00"},{"$nulls":5},"24 - 35 °",{"v":1.2,"d":"1.20"}]
[{"$nulls":7},"Groundwater in joints","Completely Dry",{"v":0.2,"d":"0.20"},{"$nulls":3},"Physical properties ","Value of c (kN/m2)","No",0]
[{"$nulls":8},"Dry",{"v":0.4,"d":"0.40"},{"$nulls":3},"of Rock slope;",null,"Lower c",{"v":0.5,"d":"0.50"}]
[{"$nulls":8},"Wet",{"v":0.6,"d":"0.60"},{"$nulls":5},"mid c",{"v":0.6,"d":"0.60"}]
[{"$nulls":8},"Dripping",{"v":0.8,"d":"0.80"},{"$nulls":5},"High c",{"v":0.7,"d":"0.70"}]
[{"$nulls":8},"Flowing",{"v":1,"d":"1.00"},{"$nulls":4},"Drill core quality (RQD); %","No",{"v":0,"d":"0.00"}]
[{"$nulls":7},"Soil depth","< 5 m",{"v":0.4,"d":"0.40"},{"$nulls":5},"90 - 100 %",{"v":0.4,"d":"0.40"}]
[{"$nulls":8},"6 – 11 m",{"v":0.6,"d":"0.60"},{"$nulls":5},"75 - 90 %",{"v":0.6,"d":"0.60"}]
[{"$nulls":8},"12 – 20 m",{"v":0.8,"d":"0.80"},{"$nulls":5},"50 - 75 %",{"v":0.8,"d":"0.80"}]
[{"$nulls":8},"> 20 m",{"v":1,"d":"1.00"},{"$nulls":5},"25 - 50 %",{"v":1,"d":"1.00"}]
[{"$nulls":15},"< 25",{"v":1.2,"d":"1.20"}]
[{"$nulls":14},"Angle of friction (degrees) (°)","No",{"v":0,"d":"0.00"}]
[{"$nulls":6},"Sub-Factor","Variable",null,"Rating",{"$nulls":5},"24 - 32°",{"v":0.8,"d":"0.80"}]
[{"$nulls":6},"Slope Condition","Height, cut (m)","0 – 5 m",{"v":0.4,"d":"0.40"},{"$nulls":5},"33 - 41°",{"v":1.2,"d":"1.20"}]
[{"$nulls":8},"5 – 10 m",{"v":0.8,"d":"0.80"},{"$nulls":5},"42 - 50°",{"v":1.4,"d":"1.40"}]
[{"$nulls":8},"10 – 20 m",{"v":1.2,"d":"1.20"}]
[{"$nulls":8},"20 – 30 m",{"v":1.6,"d":"1.60"},null,null,"Sub-Factor for Slope History"]
[{"$nulls":8},"> 30 m",{"v":2,"d":"2.00"},{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[{"$nulls":7},"Height, fill (m)","0 – 5 m",{"v":0.8,"d":"0.80"},{"$nulls":3},"Slope history",null,"No evidence of instability observed",{"v":0.5,"d":"0.50"}]
[{"$nulls":8},"5 – 15 m",{"v":1.4,"d":"1.40"},{"$nulls":5},"Evidence of possible soil creep",{"v":1,"d":"1.00"}]
[{"$nulls":8},"15 – 30 m",{"v":2,"d":"2.00"},{"$nulls":5},"Evidence of active soil creep or minor slip or rock face instability",{"v":1.5,"d":"1.50"}]
[{"$nulls":7},"Angle gradient ","0 – 5°",{"v":0.3,"d":"0.30"},{"$nulls":5},"Evidence of active or past landslip or surface failure",{"v":1.2,"d":"1.20"}]
[{"$nulls":7},"(degree) (°)","5 – 15°",{"v":0.6,"d":"0.60"}]
[{"$nulls":8},"15 – 30°",{"v":0.9,"d":"0.90"}]
[{"$nulls":8},"30 – 40°",{"v":1.2,"d":"1.20"}]
[{"$nulls":8},"40 – 60°",{"v":1.6,"d":"1.60"}]
[{"$nulls":8},"> 60°",{"v":2,"d":"2.00"}]
[{"$nulls":7},"Horizontal profile","Concave",0.15]
[{"$nulls":8},"Convex",{"v":0.2,"d":"0.20"}]
[{"$nulls":8},"Straight",0.25]
[{"$nulls":7},"Vertical profile","Down slope",{"v":0.1,"d":"0.10"}]
[{"$nulls":8},"Complex",0.15]
[{"$nulls":8},"Upslope",{"v":0.2,"d":"0.20"}]
[{"$nulls":8},"Straight",0.25]
[{"$nulls":7},"Drainage at top","None",{"v":0.5,"d":"0.50"}]
[{"$nulls":8},"Blocked",{"v":0.4,"d":"0.40"}]
[{"$nulls":8},"Fair",{"v":0.3,"d":"0.30"}]
[{"$nulls":8},"Good",{"v":0.2,"d":"0.20"}]
[{"$nulls":7},"Drainage at toe","None",{"v":0.5,"d":"0.50"}]
[{"$nulls":8},"Blocked",{"v":0.4,"d":"0.40"}]
[{"$nulls":8},"Fair",{"v":0.3,"d":"0.30"}]
[{"$nulls":8},"Good",{"v":0.2,"d":"0.20"}]
[{"$nulls":7},"Berm drainage","None",{"v":0.5,"d":"0.50"}]
[{"$nulls":8},"Blocked",{"v":0.4,"d":"0.40"}]
[{"$nulls":8},"Fair",{"v":0.3,"d":"0.30"}]
[{"$nulls":8},"Good",{"v":0.2,"d":"0.20"}]

{"sheet":"reting","index":1,"n_rows":85,"n_cols":18,"rows_kept":85,"hidden":true,"merged":[[2,1,2,4],[2,6,2,11],[2,13,2,18],[3,8,3,9],[3,15,3,16],[16,1,16,4],[16,13,16,18],[17,15,17,16],[19,6,19,11],[20,8,20,9],[24,13,24,18],[25,15,25,16],[28,6,28,11],[29,8,29,9],[50,6,50,11],[51,8,51,9],[55,13,55,18],[56,15,56,16]]}
[]
[]
[null," LHRA Factor and Max. Hazard Rating",{"$nulls":4},"Sub-Factor for Lithology",{"$nulls":6},"Sub-Factor for Erotion"]
[null,null,"Factor","Max. Hazard Rating",{"$nulls":3},"Sub-Factor","Variable",null,"Rating",{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[null,null,"Lithology",{"v":6,"d":"6.00"},{"$nulls":3},"Lithology","Rock Type","Quartzite and limestone",{"v":0.6,"d":"0.60"},{"$nulls":3},"Erotion","No appreciable erosion","No appreciable erosion",{"v":0.2,"d":"0.20"}]
[null,null,"Degree of weathering",{"v":4,"d":"4.00"},{"$nulls":5},"Granite and gabbro",{"v":0.9,"d":"0.90"},{"$nulls":4},"Sheet erosion","Minor",{"v":0.6,"d":"0.60"}]
[null,null,"Structure",{"v":4,"d":"4.00"},{"$nulls":5},"Gneiss",{"v":1.2,"d":"1.20"},{"$nulls":5},"Moderate",{"v":0.8,"d":"0.80"}]
[null,null,"Slope condition",{"v":6,"d":"6.00"},{"$nulls":5},"Well-cemented ferrigenuous sedimentary rocks,dominantly sandstones with minor beds of claystone",{"v":3,"d":"3.00"},{"$nulls":5},"Severe",{"v":1,"d":"1.00"}]
[null,null,"Hydrology",{"v":6,"d":"6.00"},{"$nulls":5},"Poorly cemented terrigenuous sedimentary rocks, dominantly sand with clayey shale beds",{"v":4,"d":"4.00"},{"$nulls":4},"Rill erosion","Minor",{"v":0.6,"d":"0.60"}]
[null,null,"Erosion",{"v":4,"d":"4.00"},{"$nulls":5},"Salt and phyllite",{"v":3.6,"d":"3.60"},{"$nulls":5},"Moderate",{"v":0.8,"d":"0.80"}]
[null,null,"Physical / engineering properties",{"v":4,"d":"4.00"},{"$nulls":5},"Schist",{"v":4,"d":"4.00"},{"$nulls":5},"Severe",{"v":1,"d":"1.00"}]
[null,null,"Land use and land cover",{"v":4,"d":"4.00"},{"$nulls":5},"Shale with interbeded sandstone and quartzite",{"v":5.4,"d":"5.40"},{"$nulls":4},"Gully erosion","Minor",{"v":1.2,"d":"1.20"}]
[null,null,"Slope history",{"v":2,"d":"2.00"},{"$nulls":5},"Highly weathered shale, phyllite and schist typically with 60% of salt",{"v":6,"d":"6.00"},{"$nulls":5},"Moderate",{"v":1.6,"d":"1.60"}]
[null,null,"Total",{"$f":"SUM(D5:D13)","v":{"v":40,"d":"40.00"}},{"$nulls":4},"Soil Type","Older well-compacted fluvial fill material (alluvial)",{"v":2.4,"d":"2.40"},{"$nulls":5},"Severe",{"v":2,"d":"2.00"}]
[{"$nulls":9},"Clayey soil with naturally formed surface (eluvial)",{"v":3,"d":"3.00"}]
[{"$nulls":9},"Sandy soil with naturally formed surface (alluvial) Debris comprising mostly rock pieces mixed with clayey / sandy soil (colluvial):",{"v":4.2,"d":"4.20"}]
[null," Hazard values and ratings ",{"$nulls":7},"Older well compacted sandy soil",{"v":5,"d":"5.00"},null,null,"Sub-Factor for Slope Cover"]
[null,null,"Hazard ratings","Hazard values",{"$nulls":5},"Younger loose material sandy soil or mining material",{"v":6,"d":"6.00"},{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[null,null,"Very High Hazard","> 32.0",{"$nulls":10},"Slope Cover",null,"Thickly vegetated area",{"v":1,"d":"1.00"}]
[null,null,"High Hazard","26.6 – 31.9",null,null,"Sub-Factor for Degree of weathering",{"$nulls":9},"Moderately vegetated area",{"v":2,"d":"2.00"}]
[null,null,"Moderate Hazard","20.4 – 26.5",{"$nulls":3},"Sub-Factor","Variable",null,"Rating",{"$nulls":5},"Artificially and vegetated area",{"v":2.2,"d":"2.20"}]
[null,null,"Low Hazard","14.1 – 20.3",{"$nulls":3},"Degree of weathering",null,"Fresh",{"v":0.6,"d":"0.60"},{"$nulls":5},"Artificial covers",{"v":2,"d":"2.00"}]
[null,null,"Very Low Hazard","< 14.0",{"$nulls":5},"Slightly weathered",{"v":1.2,"d":"1.20"},{"$nulls":5},"No cover",{"v":4,"d":"4.00"}]
[{"$nulls":9},"Moderately weathered",{"v":1.8,"d":"1.80"}]
[{"$nulls":9},"Highly weathered",{"v":2.4,"d":"2.40"},null,null,"Sub-Factor for Physical Properties"]
[{"$nulls":9},"Extremely weathered",{"v":3,"d":"3.00"},{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[{"$nulls":9},"Residual soil",{"v":4,"d":"4.00"},{"$nulls":3},"Physical properties ","Value of c (kN/m2)","No",0]
[{"$nulls":14},"of Soil slope;",null,"< 6 kN/m2",{"v":0.8,"d":"0.80"}]
[{"$nulls":6},"Sub-Factor for Structure",{"$nulls":9},"6 - 12 kN/m2",{"v":1,"d":"1.00"}]
[{"$nulls":7},"Sub-Factor","Variable",null,"Rating",{"$nulls":5},"12 - 18 kN/m2",{"v":1.2,"d":"1.20"}]
[{"$nulls":7},"Structure","Spacing of","> 2m",{"v":0.2,"d":"0.20"},{"$nulls":5},"> 18 kN/m2",{"v":1.4,"d":"1.40"}]
[{"$nulls":8},"discontinuities;","0.6m – 2m",{"v":0.4,"d":"0.40"},{"$nulls":4},"Plasticity index","No",{"v":0,"d":"0.00"}]
[{"$nulls":9},"200 mm – 600 mm",{"v":0.6,"d":"0.60"},{"$nulls":5},"< 10",{"v":0.8,"d":"0.80"}]
[{"$nulls":9},"60 mm – 200 mm",{"v":0.8,"d":"0.80"},{"$nulls":5}," 10 - 23 ",{"v":1.2,"d":"1.20"}]
[{"$nulls":9},"< 60 mm",{"v":1,"d":"1.00"},{"$nulls":5},"24 - 35",{"v":1.2,"d":"1.20"}]
[{"$nulls":8},"Width and continuity","Very rough surface. Not continuous. No separation. Unweathered wall rock.",{"v":0.2,"d":"0.20"},{"$nulls":5},"> 35 ",{"v":1.4,"d":"1.40"}]
[{"$nulls":8},"of joints","Slightly rough surface. Separation < 1mm.Slightly weathered wall.",{"v":0.4,"d":"0.40"},{"$nulls":4},"Angle of friction (degrees)","No",{"v":0,"d":"0.00"}]
[{"$nulls":9},"Slightly rough surface. Separation < 1mm.Highly weathered wall",{"v":0.6,"d":"0.60"},{"$nulls":5}," 0 - 11 °",{"v":0.8,"d":"0.80"}]
[{"$nulls":9},"Slickensided surface. OR Gouge < 5mm thick OR Separation 1 - 5mm continuous.",{"v":0.8,"d":"0.80"},{"$nulls":5},"12 - 23 °",{"v":1,"d":"1.00"}]
[{"$nulls":9},"Soft Gough > 5mm OR Separation > 5mm continuous.",{"v":1,"d":"1.00"},{"$nulls":5},"24 - 35 °",{"v":1.2,"d":"1.20"}]
[{"$nulls":8},"Groundwater in joints","Completely Dry",{"v":0.2,"d":"0.20"},{"$nulls":3},"Physical properties ","Value of c (kN/m2)","No",0]
[{"$nulls":9},"Dry",{"v":0.4,"d":"0.40"},{"$nulls":3},"of Rock slope;",null,"Lower c",{"v":0.5,"d":"0.50"}]
[{"$nulls":9},"Wet",{"v":0.6,"d":"0.60"},{"$nulls":5},"mid c",{"v":0.6,"d":"0.60"}]
[{"$nulls":9},"Dripping",{"v":0.8,"d":"0.80"},{"$nulls":5},"High c",{"v":0.7,"d":"0.70"}]
[{"$nulls":9},"Flowing",{"v":1,"d":"1.00"},{"$nulls":4},"Drill core quality (RQD); %","No",{"v":0,"d":"0.00"}]
[{"$nulls":8},"Soil depth","< 5 m",{"v":0.4,"d":"0.40"},{"$nulls":5},"90 - 100 %",{"v":0.4,"d":"0.40"}]
[{"$nulls":9},"6 – 11 m",{"v":0.6,"d":"0.60"},{"$nulls":5},"75 - 90 %",{"v":0.6,"d":"0.60"}]
[{"$nulls":9},"12 – 20 m",{"v":0.8,"d":"0.80"},{"$nulls":5},"50 - 75 %",{"v":0.8,"d":"0.80"}]
[{"$nulls":9},"> 20 m",{"v":1,"d":"1.00"},{"$nulls":5},"25 - 50 %",{"v":1,"d":"1.00"}]
[{"$nulls":16},"< 25",{"v":1.2,"d":"1.20"}]
[{"$nulls":6},"Sub-Factor for Slope Condition",{"$nulls":8},"Angle of friction (degrees) (°)","No",{"v":0,"d":"0.00"}]
[{"$nulls":7},"Sub-Factor","Variable",null,"Rating",{"$nulls":5},"24 - 32°",{"v":0.8,"d":"0.80"}]
[{"$nulls":7},"Slope Condition","Height, cut (m)","0 – 5 m",{"v":0.4,"d":"0.40"},{"$nulls":5},"33 - 41°",{"v":1.2,"d":"1.20"}]
[{"$nulls":9},"5 – 10 m",{"v":0.8,"d":"0.80"},{"$nulls":5},"42 - 50°",{"v":1.4,"d":"1.40"}]
[{"$nulls":9},"10 – 20 m",{"v":1.2,"d":"1.20"}]
[{"$nulls":9},"20 – 30 m",{"v":1.6,"d":"1.60"},null,null,"Sub-Factor for Slope History"]
[{"$nulls":9},"> 30 m",{"v":2,"d":"2.00"},{"$nulls":3},"Sub-Factor","Variable",null,"Rating"]
[{"$nulls":8},"Height, fill (m)","0 – 5 m",{"v":0.8,"d":"0.80"},{"$nulls":3},"Slope history",null,"No evidence of instability observed",{"v":0.5,"d":"0.50"}]
[{"$nulls":9},"5 – 15 m",{"v":1.4,"d":"1.40"},{"$nulls":5},"Evidence of possible soil creep",{"v":1,"d":"1.00"}]
[{"$nulls":9},"15 – 30 m",{"v":2,"d":"2.00"},{"$nulls":5},"Evidence of active soil creep or minor slip or rock face instability",{"v":1.5,"d":"1.50"}]
[{"$nulls":8},"Angle gradient ","0 – 5°",{"v":0.3,"d":"0.30"},{"$nulls":5},"Evidence of active or past landslip or surface failure",{"v":1.2,"d":"1.20"}]
[{"$nulls":8},"(degree) (°)","5 – 15°",{"v":0.6,"d":"0.60"}]
[{"$nulls":9},"15 – 30°",{"v":0.9,"d":"0.90"}]
[{"$nulls":9},"30 – 40°",{"v":1.2,"d":"1.20"}]
[{"$nulls":9},"40 – 60°",{"v":1.6,"d":"1.60"}]
[{"$nulls":9},"> 60°",{"v":2,"d":"2.00"}]
[{"$nulls":8},"Horizontal profile","Concave",0.15]
[{"$nulls":9},"Convex",{"v":0.2,"d":"0.20"}]
[{"$nulls":9},"Straight",0.25]
[{"$nulls":8},"Vertical profile","Down slope",{"v":0.1,"d":"0.10"}]
[{"$nulls":9},"Complex",0.15]
[{"$nulls":9},"Upslope",{"v":0.2,"d":"0.20"}]
[{"$nulls":9},"Straight",0.25]
[{"$nulls":8},"Drainage at top","None",{"v":0.5,"d":"0.50"}]
[{"$nulls":9},"Blocked",{"v":0.4,"d":"0.40"}]
[{"$nulls":9},"Fair",{"v":0.3,"d":"0.30"}]
[{"$nulls":9},"Good",{"v":0.2,"d":"0.20"}]
[{"$nulls":8},"Drainage at toe","None",{"v":0.5,"d":"0.50"}]
[{"$nulls":9},"Blocked",{"v":0.4,"d":"0.40"}]
[{"$nulls":9},"Fair",{"v":0.3,"d":"0.30"}]
[{"$nulls":9},"Good",{"v":0.2,"d":"0.20"}]
[{"$nulls":8},"Berm drainage","None",{"v":0.5,"d":"0.50"}]
[{"$nulls":9},"Blocked",{"v":0.4,"d":"0.40"}]
[{"$nulls":9},"Fair",{"v":0.3,"d":"0.30"}]
[{"$nulls":9},"Good",{"v":0.2,"d":"0.20"}]

{"sheet":"FORM RATING","index":2,"n_rows":122,"n_cols":14,"rows_kept":122,"merged":[[2,1,3,13],[4,11,4,13],[5,2,5,4],[5,11,5,13],[7,1,7,13],[8,2,8,4],[9,1,10,1],[9,2,9,4],[9,10,10,11],[9,12,10,13],[10,2,10,4],[12,1,12,13],[13,1,13,13],[14,4,14,12],[15,1,16,1],[17,1,17,13],[19,1,19,13],[20,1,25,1],[20,2,21,2],[22,2,23,2],[22,3,23,3],[26,1,26,13],[27,1,34,1],[35,1,35,13],[36,1,39,1],[40,1,40,13],[41,1,44,1],[45,1,45,13],[47,1,47,13],[48,1,50,1],[51,1,53,1],[54,1,54,13],[56,1,56,13],[57,1,57,4],[57,11,58,12],[57,13,58,13],[59,11,59,13],[60,11,60,13]]}
[]
[]
[null,"SLOPE HAZARD RATING RECORD"]
[]
[{"$nulls":10},"FORM 1","HAZARD RATING RECORD"]
[null,"Slope Name",{"$nulls":7},"Date"]
[]
[null,"Slope ID"]
[null,"Location",{"$nulls":8},"STA",null,"-"]
[null,"GPS Coordinate",{"$nulls":3},"S",{"$nulls":4},"Slide of Road"]
[{"$nulls":5},"E"]
[]
[null,"Slope Rating"]
[]
[null,"Factor","Sub-Factor","Choice",{"$nulls":9},"Rating"]
[null,"Lithology","Rock Type",null,"Well-cemented ferrigenuous sedimentary rocks, dominantly sandstones with minor beds of claystone",{"$nulls":8},{"$f":"IF(E16=Data!B4,\"0.6\",IF(E16=Data!B5,\"0.9\",IF(E16=Data!B6,\"1.2\",IF(E16=Data!B7,\"3\",IF(E16=Data!B8,\"4\",IF(E16=Data!B9,\"3.6\",IF(E16=Data!B10,\"4\",IF(E16=Data!B11,\"5.4\",IF(E16=Data!B12,\"6\",\"0\")))))))))","v":"3"}]
[null,null,"Soil Type",{"$nulls":10},{"$f":"IF(E17=Data!B14,\"2.4\",IF(E17=Data!B15,\"3\",IF(E17=Data!B16,\"4.2\",IF(E17=Data!B17,\"5\",IF(E17=Data!B18,\"16\",\"0\")))))","v":"0"}]
[]
[null,"Degree of weathering",null,null,"Highly weathered",{"$nulls":8},{"$f":"IF(E19=Data!B20,\"0.6\",IF(E19=Data!B21,\"1.2\",IF(E19=Data!B22,\"1.8\",IF(E19=Data!B23,\"2.4\",IF(E19=Data!B24,\"3\",IF(E19=Data!B25,\"4\",\"0\"))))))","v":"2.4"}]
[]
[null,"Structure","Spacing of discontinuities;",{"$nulls":10},{"$f":"IF(E21=Data!B27,\"0.2\",IF(E21=Data!B28,\"0.4\",IF(E21=Data!B29,\"0.6\",IF(E21=Data!B30,\"0.8\",IF(E21=Data!B31,\"1\",\"0\")))))","v":"0"}]
[]
[null,null,"Width and continuity of joints",{"$nulls":10},{"$f":"IF(E23=Data!B33,\"0.2\",IF(E23=Data!B34,\"0.4\",IF(E23=Data!B35,\"0.6\",IF(E23=Data!B36,\"0.8\",IF(E23=Data!B37,\"1\",\"0\")))))","v":"0"}]
[]
[null,null,"Groundwater in joints",{"$nulls":10},{"$f":"IF(E25=Data!B39,\"0.2\",IF(E25=Data!B40,\"0.4\",IF(E25=Data!B41,\"0.6\",IF(E25=Data!B42,\"0.8\",IF(E25=Data!B43,\"1\",\"0\")))))","v":"0"}]
[null,null,"Soil depth",{"$nulls":10},{"$f":"IF(E26=Data!B45,\"0.4\",IF(E26=Data!B46,\"0.6\",IF(E26=Data!B47,\"0.8\",IF(E26=Data!B48,\"1\",\"0\"))))","v":"0"}]
[]
[null,"Slope Condition","Height, cut (m)",null,"10 - 20 m",{"$nulls":8},{"$f":"IF(E28=Data!B50,\"0.4\",IF(E28=Data!B51,\"0.8\",IF(E28=Data!B52,\"1.2\",IF(E28=Data!B53,\"1.6\",IF(E28=Data!B54,\"2\",\"0\")))))","v":"1.2"}]
[null,null,"Height, fill (m)",{"$nulls":10},{"$f":"IF(E29=Data!B56,\"0.8\",IF(E29=Data!B57,\"1.4\",IF(E29=Data!B58,\"2\",\"0\")))","v":"0"}]
[null,null,"Angle gradient  (°)",null,"30 - 40o",{"$nulls":8},{"$f":"IF(E30=Data!B60,\"0.3\",IF(E30=Data!B61,\"0.6\",IF(E30=Data!B62,\"0.9\",IF(E30=Data!B63,\"1.2\",IF(E30=Data!B64,\"1.6\",IF(E30=Data!B65,\"2\",\"0\"))))))","v":"1.2"}]
[null,null,"Horizontal profile",null,"Straight",{"$nulls":8},{"$f":"IF(E31=Data!B67,\"0.15\",IF(E31=Data!B68,\"0.2\",IF(E31=Data!B69,\"0.25\",\"0\")))","v":"0.25"}]
[null,null,"Vertical profile",null,"Straight",{"$nulls":8},{"$f":"IF(E32=Data!B71,\"0.1\",IF(E32=Data!B72,\"0.15\",IF(E32=Data!B73,\"0.2\",IF(E32=Data!B74,\"0.25\",\"0\"))))","v":"0.25"}]
[null,null,"Drainage at top",null,"None",{"$nulls":8},{"$f":"IF(E33=Data!B76,\"0.5\",IF(E33=Data!B77,\"0.4\",IF(E33=Data!B78,\"0.3\",IF(E33=Data!B79,\"0.2\",\"0\"))))","v":"0.5"}]
[null,null,"Drainage at toe",null,"Good",{"$nulls":8},{"$f":"IF(E34=Data!B81,\"0.5\",IF(E34=Data!B82,\"0.4\",IF(E34=Data!B83,\"0.3\",IF(E34=Data!B84,\"0.2\",\"0\"))))","v":"0.2"}]
[null,null,"Berm drainage",null,"None",{"$nulls":8},{"$f":"IF(E35=Data!B86,\"0.5\",IF(E35=Data!B87,\"0.4\",IF(E35=Data!B88,\"0.3\",IF(E35=Data!B89,\"0.2\",\"0\"))))","v":"0.5"}]
[]
[null,"Hidrology","Maximum Daily Precipitation",null,"100 - 200",{"$nulls":8},{"$f":"IF(E37=Data!B91,\"0.8\",IF(E37=Data!B92,\"1\",IF(E37=Data!B93,\"1.2\",IF(E37=Data!B94,\"1.4\",IF(E37=Data!B95,\"1.6\",\"0\")))))","v":"1.2"}]
[null,null,"Maximum Hourly Precipitation",null,"> 60",{"$nulls":8},{"$f":"IF(E38=Data!B97,\"0.6\",IF(E38=Data!B98,\"0.8\",IF(E38=Data!B99,\"1\",IF(E38=Data!B100,\"1.2\",IF(E38=Data!B101,\"1.4\",\"0\")))))","v":"1.4"}]
[null,null,"Permeability",null,"Moderate to Rapid",{"$nulls":8},{"$f":"IF(E39=Data!B103,\"1.4\",IF(E39=Data!B104,\"1.2\",IF(E39=Data!B105,\"1\",IF(E39=Data!B106,\"0.8\",IF(E39=Data!B107,\"0.6\",IF(E39=Data!B108,\"0.4\",IF(E39=Data!B109,\"0.2\",\"0\")))))))","v":"1.2"}]
[null,null,"Seepage",{"$nulls":10},{"$f":"IF(E40=Data!B111,\"1.6\",IF(E40=Data!B112,\"1.4\",IF(E40=Data!B113,\"1.2\",IF(E40=Data!B114,\"1\",\"0\"))))","v":"0"}]
[]
[null,"Erotion","No Erotion",{"$nulls":10},{"$f":"IF(E42=Data!B116,\"0.2\",\"0\")","v":"0"}]
[null,null,"Sheet erosion",null,"Minor",{"$nulls":8},{"$f":"IF(E43=Data!B118,\"0.6\",IF(E43=Data!B119,\"0.8\",IF(E43=Data!B120,\"1\",\"0\")))","v":"0.6"}]
[null,null,"Rill erosion",null,"Minor",{"$nulls":8},{"$f":"IF(E43=Data!B122,\"0.6\",IF(E43=Data!B123,\"0.8\",IF(E43=Data!B124,\"1\",\"0\")))","v":"0.6"}]
[null,null,"Gully erosion",null,"Minor",{"$nulls":8},{"$f":"IF(E44=Data!B126,\"1.2\",IF(E44=Data!B127,\"1.6\",IF(E44=Data!B128,\"2\",\"0\")))","v":"1.2"}]
[]
[null,"Slope Cover",null,null,"No cover",{"$nulls":8},{"$f":"IF(E47=Data!B130,\"1\",IF(E47=Data!B131,\"2\",IF(E47=Data!B132,\"2.2\",IF(E47=Data!B133,\"2.4\",IF(E47=Data!B134,\"4\",\"0\")))))","v":"4"}]
[]
[null,"Physical properties of Soil slope;","Value of c (kN/m2)",{"$nulls":10},{"$f":"IF(E49=Data!B136,\"0.8\",IF(E49=Data!B137,\"1\",IF(E49=Data!B138,\"1.2\",IF(E49=Data!B139,\"1.4\",\"0\"))))","v":"0"}]
[null,null,"Plasticity index",{"$nulls":10},{"$f":"IF(E50=Data!B141,\"0.8\",IF(E50=Data!B142,\"1\",IF(E50=Data!B143,\"1.2\",IF(E50=Data!B144,\"1.4\",\"0\"))))","v":"0"}]
[null,null,"Angle of friction (°)",{"$nulls":10},{"$f":"IF(E51=Data!B146,\"0.8\",IF(E51=Data!B147,\"1\",IF(E51=Data!B148,\"1.2\",\"0\")))","v":"0"}]
[null,"Physical properties of Rock slope; ","Value of c (kN/m2)",null,"Lower c",{"$nulls":8},{"$f":"IF(E52=Data!B150,\"0.5\",IF(E52=Data!B151,\"0.6\",IF(E52=Data!B152,\"0.7\",\"0\")))","v":"0.5"}]
[null,null,"Drill core quality (RQD); %",null,"50 - 75",{"$nulls":8},{"$f":"IF(E53=Data!B154,\"0.4\",IF(E53=Data!B155,\"0.6\",IF(E53=Data!B156,\"0.8\",IF(E53=Data!B157,\"1\",IF(E53=Data!B158,\"1.2\",\"0\")))))","v":"0.8"}]
[null,null,"Angle of friction  (°)",null,"33 - 41o",{"$nulls":8},{"$f":"IF(E54=Data!B160,\"0.8\",IF(E54=Data!B161,\"1.2\",IF(E54=Data!B162,\"1.4\",\"0\")))","v":"1.2"}]
[]
[null,"Slope history",null,null,"No evidence",{"$nulls":8},0.5]
[]
[null," Hazard values and ratings ",{"$nulls":9},"Score",null,{"$f":"N16+N17+N19+N21+N23+N25+N26+N28+N29+N30+N31+N32+N33+N34+N35+N37+N38+N39+N40+N42+N43+N44+N45+N47+N49+N50+N51+N52+N53+N54+N56","v":22.699999999999996}]
[null,null,"Hazard ratings","Hazard values"]
[null,null,"Very High Hazard","> 32.0",{"$nulls":7},{"$f":"C59","v":"Hazard ratings"}]
[null,null,"High Hazard","26.6 – 31.9",{"$nulls":7},{"$f":"IF(N58>14,IF(N58<=20.3,C63,IF(N58<=26.5,C62,IF(N58<=31.9,C61,C60))),C64)","v":"Moderate Hazard"}]
[null,null,"Moderate Hazard","20.4 – 26.5"]
[null,null,"Low Hazard","14.1 – 20.3"]
[null,null,"Very Low Hazard","< 14.0"]
{"$rows_empty":12}
[{"$nulls":4},"Granite and gabbro",{"$nulls":8},0.9]
{"$rows_empty":14}
[{"$nulls":4},"Quartzite and limestone",{"$nulls":8},0.6]
{"$rows_empty":14}
[{"$nulls":4},"Well-cemented ferrigenuous sedimentary rocks,dominantly sandstones with minor beds of claystone",{"$nulls":8},3]
{"$rows_empty":14}
[{"$nulls":4},"Well-cemented ferrigenuous sedimentary rocks,dominantly sandstones with minor beds of claystone",{"$nulls":8},3]

{"sheet":"Data","index":3,"n_rows":167,"n_cols":2,"rows_kept":167,"hidden":true}
[]
[]
[]
[null,"Quartzite and limestone"]
[null,"Granite and gabbro"]
[null,"Gneiss"]
[null,"Well-cemented ferrigenuous sedimentary rocks, dominantly sandstones with minor beds of claystone"]
[null,"Poorly cemented terrigenuous sedimentary rocks, dominantly sand with clayey shale beds"]
[null,"Salt and phyllite"]
[null,"Schist"]
[null,"Shale with interbeded sandstone and quartzite"]
[null,"Highly weathered shale, phillite and schist typically with 60% salt"]
[]
[null,"Alluvial"]
[null,"Eluvial"]
[null,"Colluvial"]
[null,"Older well compacted sandy soil"]
[null,"Younger loose material sandy soil or mining material"]
[]
[null,"Fresh"]
[null,"Slightly weathered"]
[null,"Moderately weathered"]
[null,"Highly weathered"]
[null,"Extremely weathered"]
[null,"Residual soil"]
[]
[null,"> 2 m"]
[null,"0,6 m - 2 m"]
[null,"200 mm - 600 mm"]
[null,"60 mm - 200 mm"]
[null,"<60 mm"]
[]
[null,"Very rough surface"]
[null,"Slightly weathered wall"]
[null,"Highly weathered wall"]
[null,"Slickensided surface"]
[null,"Soft gough"]
[]
[null,"Completely dry"]
[null,"Dry"]
[null,"Wet"]
[null,"Dripping"]
[null,"Flowing"]
[]
[null,"< 5 m"]
[null,"6 -11 m"]
[null,"12 - 20 m"]
[null,"> 20 m"]
[]
[null,"0 - 5 m"]
[null,"5 - 10 m"]
[null,"10 - 20 m"]
[null,"20 - 30 m"]
[null,"> 30 m"]
[]
[null,"0 - 5 m"]
[null,"5 - 15 m"]
[null,"15 - 30 m"]
[]
[null,"0 - 5o"]
[null,"5 - 15o"]
[null,"15 - 30o"]
[null,"30 - 40o"]
[null,"40 - 60o"]
[null,"> 60o"]
[]
[null,"Concave"]
[null,"Convex"]
[null,"Straight"]
[]
[null,"Down Slope"]
[null,"Complex"]
[null,"Upslope"]
[null,"Straight"]
[]
[null,"None"]
[null,"Blocked"]
[null,"Fair"]
[null,"Good"]
[]
[null,"None"]
[null,"Blocked"]
[null,"Fair"]
[null,"Good"]
[]
[null,"None"]
[null,"Blocked"]
[null,"Fair"]
[null,"Good"]
[]
[null,"0 - 40 "]
[null,"40 - 100"]
[null,"100 - 200"]
[null,"200 - 300"]
[null,"> 300"]
[]
[null,"0 - 10"]
[null,"10 - 20"]
[null,"20 - 40"]
[null,"40 - 60"]
[null,"> 60"]
[]
[null,"Rapid"]
[null,"Moderate to Rapid"]
[null,"Slow to Moderate"]
[null,"Slow to Moderate"]
[null,"Slow"]
[null,"Very Slow"]
[null,"None"]
[]
[null,"Heavy at mid-height"]
[null,"heavy near toe"]
[null,"Slightly at mid-height"]
[null,"Slightly at toe"]
[]
[null,"No appreciable erosion"]
[]
[null,"Minor"]
[null,"Moderate"]
[null,"Severe"]
[]
[null,"Minor"]
[null,"Moderate"]
[null,"Severe"]
[]
[null,"Minor"]
[null,"Moderate"]
[null,"Severe"]
[]
[null,"Thickly vegetated area"]
[null,"Moderately vegetated area"]
[null,"Artificially and vegetated area"]
[null,"Artificial covers"]
[null,"No cover"]
[]
[null,"< 6"]
[null,"6 - 12"]
[null,"12 - 18"]
[null,"> 18"]
[]
[null,"< 10"]
[null,"10 - 23"]
[null,"24 - 35"]
[null,"> 35"]
[]
[null,"0 - 11"]
[null,"12 - 23"]
[null,"24 - 35"]
[]
[null,"Lower c"]
[null,"Mid c"]
[null,"High c"]
[]
[null,"90 - 100"]
[null,"75 - 90"]
[null,"50 - 75"]
[null,"25 - 50"]
[null,"< 25"]
[]
[null,"24 - 32o"]
[null,"33 - 41o"]
[null,"42 - 50o"]
[]
[null,"No evidence"]
[null,"Evidence of possible creep"]
[null,"Evidence of active soil creep or minor slip"]
[null,"Evidence of active or past landslip or surface failure"]

{"sheet":"Sheet2","index":4,"n_rows":32,"n_cols":20,"rows_kept":32,"hidden":true}
[]
[null,"Slope Name","Sp01","Cr01","Date",1,"munth,year","Januari 2020","Slide of Road","Hill","Soil Type","Gravel ","Condition of","Unstable","Seepege From Slope Face or Ground","Yes","Bio-Engineering Works","rees ","Failure","Landslide"]
[null,null,"Sp02","Cr02",null,2,null,"Februari 2020",null,"Valley",null,"sand","Surface","Moderate","Natural surface Runoff","No",null,"Shrubs ",null,"collapse"]
[null,null,"Sp03","Cr03",null,3,null,"Maret 2020",null,"Right",null,"Clay",null,"Stable","Ponding Water Nearby",null,null,"Grass ",null,"Rock fall"]
[null,null,"Sp04","Cr04",null,4,null,"April 2020",null,"Left",null,"Silt",{"$nulls":5},"Gunite ",null,"Rock Mass Failure"]
[null,null,"Sp05","Cr05",null,5,null,"Mei 2020",{"$nulls":3},"Peat","Ground Water","Natural spring",{"$nulls":3},"Dental Concrete",null,"Debris Flow"]
[null,null,"Sp06","Cr06",null,6,null,"Juni 2020",{"$nulls":3},"Other….",null,"Water seepage",{"$nulls":3},"Others…..",null,"Embankment Failure"]
[null,null,"Sp07","Cr07",null,7,null,"Juli 2020",{"$nulls":5},"Dry",{"$nulls":5},"Other…."]
[null,null,"Sp08","Cr08",null,8,null,"Agustus 2020",null,null,"Geologycal","Soft soil over base rock",{"$nulls":4},"Engineering Works","Gabions \n"]
[null,null,"Sp09","Cr09",null,9,null,"September 2020",null,null," Streukture","Hard rock over weak rock","Cover ","Bare ",{"$nulls":3},"Crib Wall","Month","January"]
[null,null,"Sp10","Cr10",null,10,null,"Oktober 2020",{"$nulls":3},"Other",null,"Grass + Structure ",{"$nulls":3},"Concrete Wall",null,"February"]
[null,null,"Sp11","Cr11",null,11,null,"November 2020",{"$nulls":5},"Structure",{"$nulls":3},"Cement Masonry",null,"March"]
[null,null,"Sp12","Cr12",null,12,null,"Desember 2020",null,null,"Daylight ","Yes",{"$nulls":5},"Other…..",null,"April"]
[null,null,"Sp13","Cr13",null,13,{"$nulls":4},"Structure","No","Sheet Erotion","Severe (>40% of slope area)",{"$nulls":3},"Rock Bolts ",null,"May"]
[null,null,"Sp14","Cr14",null,14,{"$nulls":4}," (planar,wedga)",null,null,"Moderate (10% - 40%)",{"$nulls":3},"Netting ",null,"June"]
[null,null,"Sp15","Cr15",null,15,{"$nulls":7},"Minor (<10%)",{"$nulls":3},"Soil Nail ",null,"July"]
[null,null,"Sp16","Cr16",null,16,{"$nulls":4},"Soft Rock","Siltstone",{"$nulls":5},"Piles",null,"August"]
[null,null,"Sp17","Cr17",null,17,{"$nulls":5},"Phylite","Rill Erotion","Severe (0.2 – 0.5m depth)",{"$nulls":3},"Other…..",null,"September"]
[null,null,"Sp18","Cr18",null,18,{"$nulls":5},"Slate",null,"Moderate (0.05 to 0.2m depth)",{"$nulls":5},"October"]
[null,null,"Sp19","Cr19",null,19,{"$nulls":5},"Clay stone",null,"Minor (< .05 m )",null,null,"Deformation","Visible",null,"November"]
[null,null,"Sp20","Cr20",null,20,{"$nulls":5},"Schist",{"$nulls":5},"obscruse",null,"December"]
[null,null,"Sp21","Cr21",null,21,{"$nulls":5},"Others…..","Guly Erotion","Severe (>one berm)",{"$nulls":3},"None"]
[null,null,"Sp22","Cr22",null,22,{"$nulls":7},"Moderate (one berm)"]
[null,null,"Sp23","Cr23",null,23,{"$nulls":4},"Hard Rock","Quartzite",null,"Minor"]
[null,null,"Sp24","Cr24",null,24,{"$nulls":5},"Granite"]
[null,null,"Sp25","Cr25",null,25,{"$nulls":5},"Gneiss ","Drainage","Available (good) "]
[null,null,"Sp26","Cr26",null,26,{"$nulls":5},"Lime stone",null,"Available (need repair) "]
[null,null,"Sp27","Cr27",null,27,{"$nulls":5},"Sand stone",null,"Not available"]
[null,null,"Sp28","Cr28",null,28,{"$nulls":5},"Dolomite"]
[null,null,"Sp29","Cr29",null,29,{"$nulls":5},"Others….."]
[null,null,"Sp30","Cr30",null,30]
[{"$nulls":5},31]